#AP6210_NVRAM_V1.2_03192013
manfid=0x2d0
prodid=0x492
vendid=0x14e4
devid=0x4343
boardtype=0x0598

# Board Revision is P307, same nvram file can be used for P304, P305, P306 and P307 as the tssi pa params used are same
#Please force the automatic RX PER data to the respective board directory if not using P307 board, for e.g. for P305 boards force the data into the following directory /projects/BCM43362/a1_labdata/boardtests/results/sdg_rev0305
boardrev=0x1307
boardnum=777
xtalfreq=26000
boardflags=0x80201
boardflags2=0x80
sromrev=3
wl0id=0x431b
macaddr=00:90:4c:07:71:12
aa2g=1
ag0=2
maxp2ga0=74
cck2gpo=0x2222
ofdm2gpo=0x44444444
mcs2gpo0=0x6666
mcs2gpo1=0x6666
pa0maxpwr=56

#P207 PA params
#pa0b0=5447
#pa0b1=-658
#pa0b2=-175

#Same PA params for P304,P305, P306, P307

pa0b0=5447
pa0b1=-607
pa0b2=-160
pa0itssit=62
pa1itssit=62


cckPwrOffset=5
ccode=0
rssismf2g=0xa
rssismc2g=0x3
rssisav2g=0x7
triso2g=0
noise_cal_enable_2g=0
noise_cal_po_2g=0
swctrlmap_2g=0x04040404,0x02020202,0x02020202,0x010101,0x1ff
temp_add=29767
temp_mult=425

btc_flags=0x6
btc_params0=5000
btc_params1=1000
btc_params6=63
